(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "+24V")
  (net 2 "GND")
  (net 3 "unconnected-(J2-Pad3)")
  (net 4 "unconnected-(J2-Pad4)")
  (net 5 "unconnected-(J2-Pad5)")
  (net 6 "unconnected-(J2-Pad6)")
  (net 7 "unconnected-(J2-Pad7)")
  (net 8 "unconnected-(J2-Pad8)")
  (net 9 "Net-(J2-Pad9)")
  (net 10 "unconnected-(J2-Pad17)")
  (net 11 "unconnected-(J2-Pad18)")
  (net 12 "unconnected-(J2-Pad19)")
  (net 13 "unconnected-(J3-Pad4)")
  (net 14 "unconnected-(J3-Pad5)")
  (net 15 "unconnected-(J3-Pad6)")
  (net 16 "unconnected-(J3-Pad8)")
  (net 17 "unconnected-(J3-Pad9)")
  (net 18 "unconnected-(J3-Pad10)")
  (net 19 "unconnected-(J3-Pad11)")
  (net 20 "unconnected-(J3-Pad12)")
  (net 21 "unconnected-(J3-Pad18)")
  (net 22 "unconnected-(J3-Pad19)")
  (net 23 "unconnected-(J3-Pad20)")
  (net 24 "Net-(J3-Pad13)")
  (net 25 "Net-(J3-Pad14)")
  (net 26 "Net-(J3-Pad15)")
  (net 27 "Net-(J3-Pad16)")
  (net 28 "Net-(J3-Pad17)")
  (net 29 "Net-(J5-Pad4)")
  (net 30 "Net-(J5-Pad5)")
  (net 31 "Net-(J5-Pad6)")
  (net 32 "unconnected-(J2-Pad13)")
  (net 33 "Net-(J2-Pad14)")
  (net 34 "Net-(J2-Pad15)")
  (net 35 "Net-(J2-Pad16)")
  (net 36 "Net-(J3-Pad2)")
  (net 37 "unconnected-(U2-Pad2)")
  (net 38 "unconnected-(U2-Pad3)")
  (net 39 "unconnected-(U2-Pad4)")
  (net 40 "unconnected-(U2-Pad5)")
  (net 41 "unconnected-(U2-Pad6)")
  (net 42 "unconnected-(U2-Pad7)")
  (net 43 "unconnected-(U2-Pad9)")
  (net 44 "unconnected-(U2-Pad10)")
  (net 45 "unconnected-(U2-Pad11)")
  (net 46 "unconnected-(U2-Pad12)")
  (net 47 "unconnected-(U2-Pad13)")
  (net 48 "unconnected-(U2-Pad14)")
  (net 49 "unconnected-(U2-Pad15)")
  (net 50 "unconnected-(J2-Pad1)")
  (net 51 "unconnected-(J2-Pad2)")
  (net 52 "Net-(J1-Pad4)")
  (net 53 "Net-(R1-Pad1)")
  (net 54 "Net-(R5-Pad2)")
  (net 55 "Net-(J2-Pad20)")
  (net 56 "Net-(J3-Pad7)")

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp 030d66b9-7057-49cb-9d71-a52d43c9b8fd)
    (at 175.758 109.245 -90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/b0751657-99dc-412f-9975-39c697d4f8ec")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f86a35ec-a627-434f-9221-034227c7e60b)
    )
    (fp_text value "Keypad" (at 0 12.49 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e94de809-2653-4e91-a70e-ed0cd58a3fe7)
    )
    (fp_text user "${REFERENCE}" (at 0 5.08) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 472be05d-223f-4cbb-aad4-7295ed6764f1)
    )
    (fp_line (start -1.33 11.49) (end 1.33 11.49) (layer "F.SilkS") (width 0.12) (tstamp 075694ad-4d63-4d18-aacd-638f8b706228))
    (fp_line (start 1.33 1.27) (end 1.33 11.49) (layer "F.SilkS") (width 0.12) (tstamp 111f74c9-b4cc-40e5-95ed-747ca2bf4243))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 309d2c7b-198a-486b-8ee4-65e9bcc7f209))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 6c73bfbc-bbb9-4a44-bf93-753ca7684fa4))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 9b1d3717-079d-4e4f-aa4c-45ffa262a0ff))
    (fp_line (start -1.33 1.27) (end -1.33 11.49) (layer "F.SilkS") (width 0.12) (tstamp dc661e37-3df7-45ab-abdd-86112ba4f6c4))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 0dafcf53-2ad7-43dc-950d-3c3fe55aa7b0))
    (fp_line (start -1.8 -1.8) (end -1.8 11.95) (layer "F.CrtYd") (width 0.05) (tstamp 3553ce6f-6d46-47ed-acc0-2161f2875eb2))
    (fp_line (start -1.8 11.95) (end 1.8 11.95) (layer "F.CrtYd") (width 0.05) (tstamp 75555a75-e6ee-4255-bad4-f9b4c2697fa9))
    (fp_line (start 1.8 11.95) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 994609f6-26e5-4001-bbe6-739462c5243e))
    (fp_line (start 1.27 11.43) (end -1.27 11.43) (layer "F.Fab") (width 0.1) (tstamp 2ec99645-1770-4db3-876f-dc0930dbc631))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 39d2ec28-4274-4a2e-9e38-276b27240760))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 90a1fa68-a89e-4da5-bac0-5e2f072c0855))
    (fp_line (start -1.27 11.43) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp a49a25cc-c6ac-49b5-8ae3-0a721c19215f))
    (fp_line (start 1.27 -1.27) (end 1.27 11.43) (layer "F.Fab") (width 0.1) (tstamp da1ea7f0-8577-4bf7-a50b-03b24f30e7af))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad13)") (pinfunction "Pin_1") (pintype "passive") (tstamp a8dc59b2-af3f-4b6c-93a1-eabb23adc7a8))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad14)") (pinfunction "Pin_2") (pintype "passive") (tstamp e383aa44-8ad7-46d5-b628-f6756cbc8a23))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad15)") (pinfunction "Pin_3") (pintype "passive") (tstamp 6cdf09fe-60d4-416c-91a1-363fe0d432e4))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad16)") (pinfunction "Pin_4") (pintype "passive") (tstamp af752199-2821-40e8-833a-f70a94d0abe3))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad17)") (pinfunction "Pin_5") (pintype "passive") (tstamp f876f61d-234b-4de1-bd83-1b0ac0bbe8c0))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 5a2f7fb5-d7d6-4369-82cc-bd6d766972f6)
    (at 164.592 129.54 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/e715b02d-2e65-4de0-ad76-fc075408f15f")
    (attr through_hole)
    (fp_text reference "R4" (at 5.08 -2.37 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b8af7bef-a384-4db0-af3d-29bdfb2e3c61)
    )
    (fp_text value "160k" (at 5.08 2.37 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4df64b56-d84a-43ce-a19c-9e37c2134445)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d0aeb901-5928-4b62-8c73-99336af392c7)
    )
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp 03cc39ea-5502-4062-ac18-fc14c283695e))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 47fb1ca7-8675-4d9f-9f69-3ccc070378e7))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 5974cab6-3ef5-46ff-b325-56c9bc777c59))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp 7379e72c-c5b6-4a1e-97a2-838ecbf12db4))
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp 7ebca9a7-856d-48bd-9b08-1a4981d2db60))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp cbb8a2ff-9d66-48d2-9523-54a026f61b51))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 32783102-9331-4cf9-a50c-14b9f820a863))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 844a21ab-d70a-404b-83b9-d45fa47d18a5))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp a0e10b86-6760-4f8c-88a3-4808fd5e3706))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp ac1fdaec-45ae-445b-8995-75106a57265d))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp 5b2da834-c5bd-43ba-9bee-81b5df7d47c8))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp 630bb28d-0c18-4b84-b40f-4036379dc860))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp 6d997fc8-6c9b-4027-b266-d0e78424fc20))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp 8f89c2a1-7eb7-4e40-ac2b-6a98ea0b9ac9))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp e1c13c74-618e-4d57-b9a0-9e45f2119397))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp f578a0d7-655d-4635-8f67-e2ae3b0ea568))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive") (tstamp 0898e6f5-1c05-48ac-b1e7-282260967d4a))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(J3-Pad7)") (pintype "passive") (tstamp 4d31edd4-c47b-4c9d-a322-d4faf7e6bf90))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type011_RT05504HBWC_1x04_P5.00mm_Horizontal" (layer "F.Cu")
    (tedit 5B294E99) (tstamp 99e7242a-1c8c-4345-b2dc-9c8086a6ac19)
    (at 206.118 113.075 180)
    (descr "terminal block Metz Connect Type011_RT05504HBWC, 4 pins, pitch 5mm, size 20x10.5mm^2, drill diamater 1.4mm, pad diameter 2.8mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_310111_RT055xxHBLC_OFF-022717S.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type011_RT05504HBWC pitch 5mm size 20x10.5mm^2 drill 1.4mm pad 2.8mm")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/56bbc9ab-9369-4297-a8cf-c4efe7e4e830")
    (attr through_hole)
    (fp_text reference "J1" (at 7.5 -7.56) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f872305a-8648-4433-be51-a23381dfab73)
    )
    (fp_text value "TCS/Power" (at 7.5 5.06) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 04c39d41-3d84-45dc-8b76-85b75c254129)
    )
    (fp_text user "${REFERENCE}" (at 7.5 3.25) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0e88073-7655-4544-b47d-4b3db08417cb)
    )
    (fp_line (start 8.7 1.083) (end 8.65 1.133) (layer "F.SilkS") (width 0.12) (tstamp 053bc9d6-13e6-44ac-b218-6a4a9945ce3f))
    (fp_line (start 3.7 1.083) (end 3.65 1.133) (layer "F.SilkS") (width 0.12) (tstamp 068f483b-7822-4c37-a7d1-7b5733d25d8e))
    (fp_line (start 11.133 -1.35) (end 11.108 -1.326) (layer "F.SilkS") (width 0.12) (tstamp 1311e589-a2af-4a4a-ba0c-cbc8e782b2ff))
    (fp_line (start -2.56 2) (end 17.561 2) (layer "F.SilkS") (width 0.12) (tstamp 13f508b8-9601-4746-8e6a-b4d5a64e21bd))
    (fp_line (start 6.133 -1.35) (end 6.108 -1.326) (layer "F.SilkS") (width 0.12) (tstamp 19e9c569-e702-4eb4-8767-e3767829bde3))
    (fp_line (start -2.56 -6.56) (end -2.56 4.06) (layer "F.SilkS") (width 0.12) (tstamp 1bc86abe-781b-457d-baa8-244a3ebe7b47))
    (fp_line (start 16.133 -1.35) (end 16.108 -1.326) (layer "F.SilkS") (width 0.12) (tstamp 2d76bc94-f02d-4640-9135-c072b9866c89))
    (fp_line (start 8.892 1.325) (end 8.868 1.35) (layer "F.SilkS") (width 0.12) (tstamp 2f441e52-0418-4c03-8da5-3dedd1816f56))
    (fp_line (start 11.35 -1.133) (end 11.301 -1.083) (layer "F.SilkS") (width 0.12) (tstamp 389909d8-3776-4448-b7f8-7b48919daad7))
    (fp_line (start 17.561 -6.56) (end 17.561 4.06) (layer "F.SilkS") (width 0.12) (tstamp 3feec924-3187-46c7-bed2-487f3d535219))
    (fp_line (start -2.56 -6.56) (end 17.561 -6.56) (layer "F.SilkS") (width 0.12) (tstamp 5db9480f-7f6f-433c-8b19-565b41589ab5))
    (fp_line (start -2.56 4.06) (end 17.561 4.06) (layer "F.SilkS") (width 0.12) (tstamp 5dbb8ce5-b357-44ac-b4e4-691d0048c6ff))
    (fp_line (start 13.892 1.325) (end 13.868 1.35) (layer "F.SilkS") (width 0.12) (tstamp 67304dfd-e9ba-457d-ae97-aaa98aef6625))
    (fp_line (start 16.35 -1.133) (end 16.301 -1.083) (layer "F.SilkS") (width 0.12) (tstamp 67ad69b5-14de-4d7b-ad7f-b29addf8c5fd))
    (fp_line (start -2.56 -2) (end 17.561 -2) (layer "F.SilkS") (width 0.12) (tstamp 6a0dfc93-c4c3-465c-a778-7e250a1320ab))
    (fp_line (start -2.56 -3) (end 17.561 -3) (layer "F.SilkS") (width 0.12) (tstamp 6a562180-359a-431c-b029-07b46f5d5386))
    (fp_line (start -2.8 4.3) (end -0.8 4.3) (layer "F.SilkS") (width 0.12) (tstamp 9d8d9180-6c22-4c53-9426-585ea341fc61))
    (fp_line (start 6.35 -1.133) (end 6.301 -1.083) (layer "F.SilkS") (width 0.12) (tstamp affea506-d65d-4471-b2bd-5388ae0bbd80))
    (fp_line (start 3.892 1.325) (end 3.868 1.35) (layer "F.SilkS") (width 0.12) (tstamp ce879c42-6dad-411a-9a1f-ed52f89da30c))
    (fp_line (start -2.8 2.06) (end -2.8 4.3) (layer "F.SilkS") (width 0.12) (tstamp cfba5c6a-6f0c-47f4-8ef6-0e7e4b128827))
    (fp_line (start 13.7 1.083) (end 13.65 1.133) (layer "F.SilkS") (width 0.12) (tstamp e672c1b7-5585-4e2d-8607-939194eb67eb))
    (fp_arc (start -1.639206 0.695516) (mid -1.780657 -0.000263) (end -1.639 -0.696) (layer "F.SilkS") (width 0.12) (tstamp 14205c9f-ebe4-4a6f-b02e-50774ce55c74))
    (fp_arc (start 0.695501 1.638499) (mid 0.354875 1.744266) (end 0 1.78) (layer "F.SilkS") (width 0.12) (tstamp 517f1aac-1ad3-4232-90c7-60054fdcf88e))
    (fp_arc (start 0.030814 1.78039) (mid -0.340023 1.747891) (end -0.696 1.639) (layer "F.SilkS") (width 0.12) (tstamp 66ea3e98-284c-45ea-a1fc-ba370b0f7edf))
    (fp_arc (start 1.639206 -0.695516) (mid 1.780657 0.000263) (end 1.639 0.696) (layer "F.SilkS") (width 0.12) (tstamp cebff79d-2131-44ff-ad94-03fe7a795ba4))
    (fp_arc (start -0.695516 -1.639206) (mid 0.000263 -1.780657) (end 0.696 -1.639) (layer "F.SilkS") (width 0.12) (tstamp f52f9479-3f39-46ca-906b-020edf556955))
    (fp_circle (center 10 0) (end 11.78 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp dc1b3498-f45a-432b-b6fd-39ac96fc1727))
    (fp_circle (center 15 0) (end 16.78 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp f1bbe662-44ed-48bd-8f7d-75c37f618ab6))
    (fp_circle (center 5 0) (end 6.78 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp fc2f9925-59ad-418e-bfa3-755e1ab256ba))
    (fp_line (start -3 4.5) (end 18 4.5) (layer "F.CrtYd") (width 0.05) (tstamp 099afe7e-7fdd-41fe-b4d1-dfbda69a46a7))
    (fp_line (start 18 -7) (end -3 -7) (layer "F.CrtYd") (width 0.05) (tstamp 432513a0-2712-4de7-a152-cb8863937be7))
    (fp_line (start 18 4.5) (end 18 -7) (layer "F.CrtYd") (width 0.05) (tstamp 8641e6dc-e655-4bb2-9f73-9321c2722c4b))
    (fp_line (start -3 -7) (end -3 4.5) (layer "F.CrtYd") (width 0.05) (tstamp efc93a91-d052-4fe7-807e-2075ac59abc7))
    (fp_line (start 1.214 -1.019) (end -1.019 1.214) (layer "F.Fab") (width 0.1) (tstamp 14be6a0a-2719-47d2-93ad-ac56d2aa519e))
    (fp_line (start -2.5 -2) (end 17.5 -2) (layer "F.Fab") (width 0.1) (tstamp 2496390f-a547-4fee-a682-fbde598737be))
    (fp_line (start 16.214 -1.019) (end 13.982 1.214) (layer "F.Fab") (width 0.1) (tstamp 41ae0bd2-0406-4542-98ea-d3553ca75916))
    (fp_line (start -2.5 -3) (end 17.5 -3) (layer "F.Fab") (width 0.1) (tstamp 7549aeb7-ec81-4344-9c42-5b72c2c14f44))
    (fp_line (start -2.5 2) (end -2.5 -6.5) (layer "F.Fab") (width 0.1) (tstamp 7a8a5255-57f1-4fff-90e9-f3a5732eecd0))
    (fp_line (start 17.5 4) (end -0.5 4) (layer "F.Fab") (width 0.1) (tstamp 812c5856-c2ad-4f75-96d4-8d5a4feac60e))
    (fp_line (start 16.019 -1.214) (end 13.787 1.018) (layer "F.Fab") (width 0.1) (tstamp ae0a0abb-4c1c-4e8c-89b4-2e96e42fb485))
    (fp_line (start -2.5 -6.5) (end 17.5 -6.5) (layer "F.Fab") (width 0.1) (tstamp c3108c7a-ac29-4c39-8324-098b4ff1b029))
    (fp_line (start 11.214 -1.019) (end 8.982 1.214) (layer "F.Fab") (width 0.1) (tstamp c98bfd51-42bb-4d17-88b5-f98ad230a0e3))
    (fp_line (start 6.214 -1.019) (end 3.982 1.214) (layer "F.Fab") (width 0.1) (tstamp cbcf8e3b-1b49-4339-9d41-fb8c92fd7fe9))
    (fp_line (start 17.5 -6.5) (end 17.5 4) (layer "F.Fab") (width 0.1) (tstamp d461d4e4-de88-41b0-85de-6a2109b5208a))
    (fp_line (start -2.5 2) (end 17.5 2) (layer "F.Fab") (width 0.1) (tstamp d4744a5d-b3e7-4b1f-b8da-7a443e0c25b1))
    (fp_line (start 6.019 -1.214) (end 3.787 1.018) (layer "F.Fab") (width 0.1) (tstamp df220e51-e3d7-4d8f-ae85-0cafae19fbba))
    (fp_line (start -0.5 4) (end -2.5 2) (layer "F.Fab") (width 0.1) (tstamp e4c83963-d9c4-4874-8371-4e3b87fd61ad))
    (fp_line (start 11.019 -1.214) (end 8.787 1.018) (layer "F.Fab") (width 0.1) (tstamp ed40e786-7fbd-4325-a963-5639734bc4a3))
    (fp_line (start 1.019 -1.214) (end -1.214 1.018) (layer "F.Fab") (width 0.1) (tstamp f96eb2bb-5633-4b27-b5ac-622b035d77b4))
    (fp_circle (center 10 0) (end 11.6 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 00d7e544-a34c-47eb-b7d1-58da011ff4f8))
    (fp_circle (center 15 0) (end 16.6 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 20450633-171e-4dac-8f3c-94ba0b4b4c42))
    (fp_circle (center 5 0) (end 6.6 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp f31ac9e9-97d6-443c-84bf-9de62265bff3))
    (fp_circle (center 0 0) (end 1.6 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp f6b65a38-0b6b-4413-9c47-f22d3908ca87))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "+24V") (pinfunction "Pin_1") (pintype "passive") (tstamp bf5af867-268e-4148-9fa8-4d523f02800c))
    (pad "2" thru_hole circle (at 5 0 180) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp 7f4be8f4-5187-4032-b146-1a67605e4bd9))
    (pad "3" thru_hole circle (at 10 0 180) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive") (tstamp 277da800-eb7c-47e7-b76b-50b473a6ab98))
    (pad "4" thru_hole circle (at 15 0 180) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 52 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 00d269ad-bbda-4777-9e91-84da2b86883c))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type011_RT05504HBWC_1x04_P5.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x20_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A41E) (tstamp 9a84e48b-476c-4921-991a-d11786b777e1)
    (at 206.238 103.657 -90)
    (descr "Through hole straight socket strip, 1x20, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x20 2.54mm single row")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/7b781551-b0a2-4a9a-81b1-1844c7117d7d")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0af40c8d-1e84-4fa1-a79e-f90a3a846c6e)
    )
    (fp_text value "Conn_01x20_Male" (at 0 51.03 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 74db4471-b31f-49dc-a52d-9474c3c8974f)
    )
    (fp_text user "${REFERENCE}" (at 0 24.13) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3e49fa28-b3ac-4518-8a3e-e840e5b4e6ab)
    )
    (fp_line (start -1.33 49.59) (end 1.33 49.59) (layer "F.SilkS") (width 0.12) (tstamp 1228d699-9fd5-4911-8e2e-23ca6d443800))
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 253055ca-ea3d-4a36-87d2-18a4bc81183d))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 339f905f-30cf-4872-8fdb-28b4b758e45e))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 9e8c9062-c867-480e-ba8c-2301d1bd1d38))
    (fp_line (start -1.33 1.27) (end -1.33 49.59) (layer "F.SilkS") (width 0.12) (tstamp e9b2415f-9cc8-4447-8130-c62d9a32c5c0))
    (fp_line (start 1.33 1.27) (end 1.33 49.59) (layer "F.SilkS") (width 0.12) (tstamp f14f3d53-dc46-41fd-b15c-664dd19c9de2))
    (fp_line (start 1.75 50) (end -1.8 50) (layer "F.CrtYd") (width 0.05) (tstamp 12b722f5-e2ff-4f93-a8f4-969e67699220))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 3809325b-1e59-4d93-9560-89af48339261))
    (fp_line (start 1.75 -1.8) (end 1.75 50) (layer "F.CrtYd") (width 0.05) (tstamp 3a55d361-f946-4078-bc80-29325cfdf97e))
    (fp_line (start -1.8 50) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c8b8c8ed-ced5-4dc0-894c-bb0833823a7e))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 42c2b8fe-c117-4581-8e5c-bb02dffc7194))
    (fp_line (start 1.27 49.53) (end -1.27 49.53) (layer "F.Fab") (width 0.1) (tstamp a733c100-efc9-4109-a60b-a51c55bf7f0b))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp b8560343-d391-4036-bddf-75bb704ddadc))
    (fp_line (start 1.27 -0.635) (end 1.27 49.53) (layer "F.Fab") (width 0.1) (tstamp d7a88773-9075-4ae3-a7d6-4a199a5e64d0))
    (fp_line (start -1.27 49.53) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp e7eb5ea0-04c3-4b7f-a967-569e2d61d233))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+24V") (pinfunction "Pin_1") (pintype "passive") (tstamp d8cc9136-65e0-4a4e-82df-dda0a5feaf67))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 69883529-6608-4e24-b893-90486c280fed))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive") (tstamp ca34a34f-b562-4b98-b7e4-b9f28e2bed0f))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 9e709c1f-995f-4eea-8f9f-461b279dbde4))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J3-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp 04541df9-f5ef-4c2e-a1c5-8d0617d6881c))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "unconnected-(J3-Pad6)") (pinfunction "Pin_6") (pintype "passive") (tstamp 2469168c-4036-4251-a72b-56be9c53164a))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J3-Pad7)") (pinfunction "Pin_7") (pintype "passive") (tstamp c6d9b9a2-28de-4343-b3f1-d3cfa3c7dc6a))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(J3-Pad8)") (pinfunction "Pin_8") (pintype "passive") (tstamp 138b304f-13a8-43a8-8aa0-b96eec5fba17))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J3-Pad9)") (pinfunction "Pin_9") (pintype "passive") (tstamp d2ab0838-9525-4e69-a2b9-1ca3717de9d8))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(J3-Pad10)") (pinfunction "Pin_10") (pintype "passive") (tstamp 4dd84fda-1b40-417f-961b-8a42aebd725c))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J3-Pad11)") (pinfunction "Pin_11") (pintype "passive") (tstamp 265cd132-af5e-4392-883b-29574242c672))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(J3-Pad12)") (pinfunction "Pin_12") (pintype "passive") (tstamp 440aec5e-c2d6-40c8-9189-fa9f26332aea))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad13)") (pinfunction "Pin_13") (pintype "passive") (tstamp ed684e07-9d93-4c9a-9790-fded39047553))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad14)") (pinfunction "Pin_14") (pintype "passive") (tstamp c519d783-6fef-4db9-9dd5-e182833a3e93))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad15)") (pinfunction "Pin_15") (pintype "passive") (tstamp 5be431c8-d0ef-4bcd-9557-460777fdd60a))
    (pad "16" thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad16)") (pinfunction "Pin_16") (pintype "passive") (tstamp afef1d80-2018-4fcb-bdbe-4d80f7e4a125))
    (pad "17" thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad17)") (pinfunction "Pin_17") (pintype "passive") (tstamp fa04bd50-4f8d-4485-895b-e6db38953486))
    (pad "18" thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J3-Pad18)") (pinfunction "Pin_18") (pintype "passive") (tstamp 4da5a285-801c-42cf-8383-8f85dd6ea961))
    (pad "19" thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J3-Pad19)") (pinfunction "Pin_19") (pintype "passive") (tstamp 6a2ec772-69a0-4257-b41c-cbab62b8dfe7))
    (pad "20" thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J3-Pad20)") (pinfunction "Pin_20") (pintype "passive") (tstamp 32f318eb-525a-4f0d-b668-3e90ad81eb54))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x20_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A41E) (tstamp aabea116-9614-4995-aaf7-b5a35f91c262)
    (at 206.238 85.877 -90)
    (descr "Through hole straight socket strip, 1x20, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x20 2.54mm single row")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/becf7bdd-5a1f-4e17-b130-b4872a342dd9")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 41f6eb76-6aaa-4368-9893-e8fcf4b46426)
    )
    (fp_text value "Conn_01x20_Male" (at 0 51.03 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4fa41aaa-e7f2-4935-8316-41a3044b33e2)
    )
    (fp_text user "${REFERENCE}" (at 0 24.13) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8d106ef7-60dd-48b8-946f-bca5585e693c)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 02c6a466-0f4d-444f-b115-ce1248e3faf2))
    (fp_line (start -1.33 1.27) (end -1.33 49.59) (layer "F.SilkS") (width 0.12) (tstamp 3086943e-9477-44ab-af97-4de582956b68))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp ac147a5f-c6e5-40f9-b4c2-6c884279a104))
    (fp_line (start 1.33 1.27) (end 1.33 49.59) (layer "F.SilkS") (width 0.12) (tstamp b7028dbd-2f5f-46a5-a1c8-fd20bad54955))
    (fp_line (start -1.33 49.59) (end 1.33 49.59) (layer "F.SilkS") (width 0.12) (tstamp f5f5e0dc-6ccb-4c95-b201-591861f6da1e))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp f87315ab-4fed-430e-b830-5a7e0f3a844a))
    (fp_line (start 1.75 -1.8) (end 1.75 50) (layer "F.CrtYd") (width 0.05) (tstamp 0873bcf2-f436-4e30-98f0-58dc235053a3))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 1a5e16f7-9f30-4b30-9f2a-add814462ee4))
    (fp_line (start -1.8 50) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 284338bb-0144-4649-bbd4-483033a9f3b5))
    (fp_line (start 1.75 50) (end -1.8 50) (layer "F.CrtYd") (width 0.05) (tstamp 547438a0-2171-44cd-af78-fec4d6edf4e8))
    (fp_line (start 1.27 49.53) (end -1.27 49.53) (layer "F.Fab") (width 0.1) (tstamp 39bffa96-1fed-4c18-b940-6082325e4c76))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 59950ed6-6b32-48f0-98cf-9e0de97cc064))
    (fp_line (start 1.27 -0.635) (end 1.27 49.53) (layer "F.Fab") (width 0.1) (tstamp bcf74303-f76a-4c5a-820b-3c0275e75644))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp e8377a8d-b4bd-499c-854f-7d9129f01ab4))
    (fp_line (start -1.27 49.53) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp f367f644-bd84-47aa-aea0-66101772c46c))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "unconnected-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 453e5837-777c-4274-baf2-6a35bff3d2d9))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "unconnected-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp eb72fe11-50b7-474c-b147-890e4149c6f2))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive") (tstamp b81539b8-d442-459f-b28b-df737dee78c3))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 722aadaf-f43d-45c6-be76-12f1c3cac0fa))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "unconnected-(J2-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp 8b8bcc6d-501d-4ed9-b470-aaeab94e5fe3))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "unconnected-(J2-Pad6)") (pinfunction "Pin_6") (pintype "passive") (tstamp f1ef91cf-8366-44a7-a831-ca59b780ef8c))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(J2-Pad7)") (pinfunction "Pin_7") (pintype "passive") (tstamp 12de3d05-192a-4aba-8cc3-9c11c7748f72))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "unconnected-(J2-Pad8)") (pinfunction "Pin_8") (pintype "passive") (tstamp 0e4adb2b-8541-4513-8978-13c8b4e9a6a0))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad9)") (pinfunction "Pin_9") (pintype "passive") (tstamp 6d477048-ca00-4c85-b1ae-f5298b23cac5))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J5-Pad4)") (pinfunction "Pin_10") (pintype "passive") (tstamp 88faff30-42b3-46e4-9fa7-a966a3732316))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-Pad5)") (pinfunction "Pin_11") (pintype "passive") (tstamp 097eb5f2-0cb2-4eb3-8825-96cfb0770596))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad6)") (pinfunction "Pin_12") (pintype "passive") (tstamp 4ff41860-6b53-42bb-86f3-a8c859546f52))
    (pad "13" thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "unconnected-(J2-Pad13)") (pinfunction "Pin_13") (pintype "passive") (tstamp a9478f09-bc39-4dff-9a94-e4905ea5fc35))
    (pad "14" thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad14)") (pinfunction "Pin_14") (pintype "passive") (tstamp 0590c81d-2c48-4f9c-a2b9-b390022a8fd5))
    (pad "15" thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad15)") (pinfunction "Pin_15") (pintype "passive") (tstamp e588f32c-85f3-4cbd-ba29-e0ec9be9ce93))
    (pad "16" thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad16)") (pinfunction "Pin_16") (pintype "passive") (tstamp 055c1dbe-424a-41bf-9194-eaedc0facd19))
    (pad "17" thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(J2-Pad17)") (pinfunction "Pin_17") (pintype "passive") (tstamp ee1d7e89-1e45-4f9b-a59f-9f8c53d865f0))
    (pad "18" thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(J2-Pad18)") (pinfunction "Pin_18") (pintype "passive") (tstamp 26fd9ca0-0a35-42b5-ba16-431bd36ec2a5))
    (pad "19" thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(J2-Pad19)") (pinfunction "Pin_19") (pintype "passive") (tstamp a5bf65d3-fc70-4e1c-a6ca-823beac87a0b))
    (pad "20" thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J2-Pad20)") (pinfunction "Pin_20") (pintype "passive") (tstamp 023205cb-68e1-49d8-9dee-c7f57abad074))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5) (tstamp be1113cd-2a43-4746-b18e-04f4ed0d0288)
    (at 151.892 109.474)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/3337c503-be65-4ddc-8a0b-eb843d5e5e20")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d3445a7-b7a4-4a09-948b-5601bb61e9e0)
    )
    (fp_text value "ULN2003" (at 3.81 20.11) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8c936fcd-55bd-48f0-bd93-70ec358e592b)
    )
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d682c0a-a826-4c3b-82bc-a19d2ab4a008)
    )
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 0d99db0d-7ff7-4f37-83f4-26cdeaa4804f))
    (fp_line (start 1.16 19.11) (end 6.46 19.11) (layer "F.SilkS") (width 0.12) (tstamp 42b67ff6-19ec-4101-9428-9bf8b6ae24d2))
    (fp_line (start 6.46 19.11) (end 6.46 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 591e7d28-5fd6-4d80-ac76-f7d19486345e))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 70b19415-56e2-4848-9310-09af1990317f))
    (fp_line (start 1.16 -1.33) (end 1.16 19.11) (layer "F.SilkS") (width 0.12) (tstamp a3357161-ea7c-4e8b-a553-3ee50b3fc980))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33) (layer "F.SilkS") (width 0.12) (tstamp e30f7c04-e49a-4044-9b16-ad669a9c03f5))
    (fp_line (start -1.1 -1.55) (end -1.1 19.3) (layer "F.CrtYd") (width 0.05) (tstamp 585b372d-83a3-46cf-b0b7-1530db41c028))
    (fp_line (start 8.7 19.3) (end 8.7 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp c606c8d9-1cf9-41a4-abc7-f85387812505))
    (fp_line (start -1.1 19.3) (end 8.7 19.3) (layer "F.CrtYd") (width 0.05) (tstamp ec92e6c4-48c2-4d10-a5ce-5c21d15b2ac6))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55) (layer "F.CrtYd") (width 0.05) (tstamp ff20c0b1-2e80-4627-9d5e-7fcdca2cb679))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27) (layer "F.Fab") (width 0.1) (tstamp 588ea027-0b62-4b41-bc1d-0e02adc53676))
    (fp_line (start 0.635 19.05) (end 0.635 -0.27) (layer "F.Fab") (width 0.1) (tstamp 7a82afc5-f1d6-4cf2-a642-065acfdaf302))
    (fp_line (start 6.985 19.05) (end 0.635 19.05) (layer "F.Fab") (width 0.1) (tstamp 8b4c3619-e77d-4355-84f5-339e532464f3))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp a9bd8b27-729c-4e78-893b-e6243588266d))
    (fp_line (start 6.985 -1.27) (end 6.985 19.05) (layer "F.Fab") (width 0.1) (tstamp ea702f83-e694-402c-9fb3-5ab247fe68a3))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(R5-Pad2)") (pinfunction "I1") (pintype "input") (tstamp 5233e2a5-7ef0-4f47-a7da-20d407a559ec))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "unconnected-(U2-Pad2)") (pinfunction "I2") (pintype "input") (tstamp bf4cee40-e1cf-46dc-9fdd-07a402e455c8))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "unconnected-(U2-Pad3)") (pinfunction "I3") (pintype "input") (tstamp a5093b9a-d51f-4ca3-b1d8-6a02425619ca))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "unconnected-(U2-Pad4)") (pinfunction "I4") (pintype "input") (tstamp a200a4d3-9665-4043-a813-92ae0025f3b7))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "unconnected-(U2-Pad5)") (pinfunction "I5") (pintype "input") (tstamp 47d77db3-bda3-4e1f-855b-67ee0c841826))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "unconnected-(U2-Pad6)") (pinfunction "I6") (pintype "input") (tstamp 370f27f0-0356-4cab-8023-da43421cd0ef))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "unconnected-(U2-Pad7)") (pinfunction "I7") (pintype "input") (tstamp 93182673-de49-4159-b4a2-6579e36827f6))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 2cb60fb7-d719-4a4d-b851-722c930ca0fc))
    (pad "9" thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "unconnected-(U2-Pad9)") (pinfunction "COM") (pintype "passive") (tstamp d3b7e497-7483-4910-b9ec-b8b58c1f4577))
    (pad "10" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "unconnected-(U2-Pad10)") (pinfunction "O7") (pintype "open_collector") (tstamp 9efe824b-0ee2-4437-a99e-c8c31e6e221a))
    (pad "11" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "unconnected-(U2-Pad11)") (pinfunction "O6") (pintype "open_collector") (tstamp 23ae2236-b1af-4d9e-a09a-e08a26041aa5))
    (pad "12" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "unconnected-(U2-Pad12)") (pinfunction "O5") (pintype "open_collector") (tstamp 4be1b79d-602a-4554-bce0-0a411b52b8a8))
    (pad "13" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "unconnected-(U2-Pad13)") (pinfunction "O4") (pintype "open_collector") (tstamp 8aac2cc0-4906-45bc-a3b5-af22a462d6da))
    (pad "14" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "unconnected-(U2-Pad14)") (pinfunction "O3") (pintype "open_collector") (tstamp 632e871c-995c-4ad1-8ace-3c549e5c6ae2))
    (pad "15" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "unconnected-(U2-Pad15)") (pinfunction "O2") (pintype "open_collector") (tstamp b7a29adb-b3c6-4a46-8472-ab314d40da6f))
    (pad "16" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(R1-Pad1)") (pinfunction "O1") (pintype "open_collector") (tstamp 2aebf758-aa45-404a-9141-d4b303573c3a))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp c1683a4b-98bc-4ef7-897b-a710c9467f10)
    (at 172.466 118.11)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/26697356-fc66-4927-a9bd-9b95fd59e9ed")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.37) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6fde7fa8-135a-46b4-85d7-02207d8c8d64)
    )
    (fp_text value "1,2 Ohm" (at 5.08 -2.794) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 10d72a9f-fc07-4b39-a505-d8f70903ebfb)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dc67b8da-e194-4a10-a8b3-6e03360f0d87)
    )
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp 1208a20a-eb08-4480-9ae6-4ab9127d0a6b))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp 4546553a-3b7a-4f32-baa3-92117168d449))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp 58e5416e-8ebf-4022-b9d2-e3246c784ae3))
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp 9baa5a14-a814-4823-a1a5-1c5d8872cbeb))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 9c6988c6-ea14-444b-b3f2-a6aa4a9f6a1a))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp b550dd10-75d2-4fed-a44d-4c98a0dca39d))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 162aeda2-c4f5-45b1-8526-bd81eda7024d))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 18d0b48a-81d2-4851-9043-29ea264808d5))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp e0b39d89-f013-46b4-b2ae-a8a714371ab5))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp fc02c1a5-a92e-4797-95df-c66214f5ccf8))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp 07aa2a7c-0fba-436a-87a9-ff2948c93a17))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp 318c035a-1bc6-430c-9934-f0644cb1d4c4))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp 6122ebca-ac1b-41bf-a974-dfcaa965c0bc))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp 8f0b63e9-01f0-40b1-8d4b-f16243df6fb6))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp f452f52e-2bc9-4d66-9cd9-49781b32315d))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp f6fe1524-0819-4e63-8c72-c55daa71ba30))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(R1-Pad1)") (pintype "passive") (tstamp 2e9f3eb2-9253-4878-b60d-5f7a3b8ec9a2))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(J1-Pad4)") (pintype "passive") (tstamp e83d41e1-d8ea-48b4-ab29-848bfe66989e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x09_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A431) (tstamp c5aeced8-8228-4e03-848f-ac22bf0e10ec)
    (at 188.458 80.543 -90)
    (descr "Through hole straight socket strip, 1x09, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x09 2.54mm single row")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/6187e9be-0d47-422b-8705-6be28d327e16")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.77 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1ab3ee21-5955-4341-8057-d3ebc012b28d)
    )
    (fp_text value "Display" (at 0 23.09 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 49140e9d-6fab-40ca-ab8b-c202472abf9e)
    )
    (fp_text user "${REFERENCE}" (at 0 10.16) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 96c169ea-8e95-403b-9e16-2623f3d8b390)
    )
    (fp_line (start 0 -1.33) (end 1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 547d196f-7a55-4247-b778-b54d363fa8d8))
    (fp_line (start 1.33 -1.33) (end 1.33 0) (layer "F.SilkS") (width 0.12) (tstamp 9720cf50-9040-4ccb-8ffa-783a4142a7a8))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp a1352e9d-3d0b-415d-9ec2-f8f6f9ec54c5))
    (fp_line (start -1.33 21.65) (end 1.33 21.65) (layer "F.SilkS") (width 0.12) (tstamp d6a34f8f-7aca-4f7a-b042-69010d1704a5))
    (fp_line (start -1.33 1.27) (end -1.33 21.65) (layer "F.SilkS") (width 0.12) (tstamp e347f055-10dd-4886-8917-29a25639214a))
    (fp_line (start 1.33 1.27) (end 1.33 21.65) (layer "F.SilkS") (width 0.12) (tstamp ea447493-5528-45a3-89d4-36de7045d261))
    (fp_line (start -1.8 22.1) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 575395bf-0137-4b07-80e7-9a26ff62716a))
    (fp_line (start 1.75 22.1) (end -1.8 22.1) (layer "F.CrtYd") (width 0.05) (tstamp bccf37bb-9e69-4120-b597-2def262a22ed))
    (fp_line (start -1.8 -1.8) (end 1.75 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp ea70fe5d-dc1a-457a-845a-045efc8c1cc7))
    (fp_line (start 1.75 -1.8) (end 1.75 22.1) (layer "F.CrtYd") (width 0.05) (tstamp f39f5bc4-0de0-4418-9fd0-a090231fd1d0))
    (fp_line (start -1.27 21.59) (end -1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 33cd945b-c274-40d9-847c-657d118b8543))
    (fp_line (start 1.27 21.59) (end -1.27 21.59) (layer "F.Fab") (width 0.1) (tstamp 9afe60db-2634-4809-b269-0de516d331e8))
    (fp_line (start 1.27 -0.635) (end 1.27 21.59) (layer "F.Fab") (width 0.1) (tstamp ccb462ff-d96f-40f2-93f0-8ce3a6f05758))
    (fp_line (start 0.635 -1.27) (end 1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp d349fff7-424e-43d3-a4f2-cdee9ca1981f))
    (fp_line (start -1.27 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp ec7daa12-8237-4e6f-996f-7e0560d3f65e))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp bb62574e-7ff1-49a7-958f-e5972485cf5c))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp fa390806-8ac1-48a1-9562-bb847a2f1c00))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad9)") (pinfunction "Pin_3") (pintype "passive") (tstamp 0be20ea6-8a6f-4c17-85c0-3c34a26dc24f))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J5-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 4a0e1e45-970d-4ccc-baf8-dce9773ddcc1))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp e087b44f-6364-4635-9e4b-a3eaa48c7d4a))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad6)") (pinfunction "Pin_6") (pintype "passive") (tstamp f9915da2-7a11-4dcd-b877-f5dfe00b58e5))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad14)") (pinfunction "Pin_7") (pintype "passive") (tstamp 5640e1bb-e627-4265-824b-22b04c2d2a81))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad15)") (pinfunction "Pin_8") (pintype "passive") (tstamp 30d2ee4f-2c89-4b9c-9927-b7983c626b1f))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad16)") (pinfunction "Pin_9") (pintype "passive") (tstamp c25acad9-12c7-4900-8e28-0da84e728035))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x09_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp cff6bf92-4ce3-4661-a143-d709a553218d)
    (at 172.466 127.762)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/b8139462-0c07-4c9e-afce-4be07fb126d6")
    (attr through_hole)
    (fp_text reference "R3" (at 5.08 -2.37) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5d151879-41ef-4e5a-9041-90f2eb50a5e3)
    )
    (fp_text value "1M" (at 5.08 2.37) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ee40875a-e6c0-403c-9459-5b98e6c6110e)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 72e126ea-d03e-4204-b1e2-55cf3fb6cac9)
    )
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 0aa00d95-095b-4beb-a86b-ed9ca87e5c26))
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp 5cfe6109-dac8-4c22-98df-d3523c385df9))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp 72da2feb-013d-4039-ac5e-8f1b55f04e7d))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp a1bb20ca-8361-4d36-a463-35f6a5e75dd1))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp abff20ff-2c8d-48ac-a097-68b84267cd00))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp ac851459-ca67-4856-8217-62deb2e1e9dd))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp bcb01b26-b2af-4c3b-8cb7-cdcbbcc27092))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp c6c794a8-a37f-4ccc-9b93-99552402f73e))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp dfcf0775-b0f2-4768-a7af-efaed07718ef))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp f524840a-20f8-4f6f-b292-c5cc9684ffa5))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp 342c72a5-9e0b-4f1c-8332-cc0ec0ddcaa6))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp 5012d5e8-93dc-4529-8dee-a2e5de9c5a5b))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp 60ae6cb9-e810-4ebd-aac4-1f336a188da6))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp bcec0cf6-860e-420c-9f20-ac0d5c82edc9))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp cee2dc34-0fbc-4ecc-b889-12fc9411cd75))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp ddef6227-6e6e-49dc-92c0-079badfb9ecb))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(J3-Pad7)") (pintype "passive") (tstamp adff7884-7b11-4417-b4f7-7343833172c1))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(J1-Pad4)") (pintype "passive") (tstamp 7373fc17-8d58-48e5-8c55-523c0cb6398e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp dfa92f9b-2bdb-444d-b895-b762ed48daff)
    (at 153.162 89.662 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/f8c1173d-308f-480c-b5d8-345792d8f8a1")
    (attr through_hole)
    (fp_text reference "R5" (at 5.08 -2.37 90) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 95ef387d-dcad-40b9-8469-d572d5955d5d)
    )
    (fp_text value "1k" (at 5.08 -2.794 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61eb9cd5-6ff1-4454-b474-de319ae6d60f)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 89778e1a-21d5-49cb-88d1-a9079af47ccd)
    )
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp 25da846b-cd31-4601-a9bb-f234cee5740f))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp 4f5d0cfe-ee6f-4759-9103-f7bdd35e13a5))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 60fe7026-f5cc-4f44-9eb2-6b1b5ce76185))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp a5ecb977-bd5c-498b-93ce-aecfa9f35c3c))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp a97fc570-221a-4d24-92fd-a5e22c227eff))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp f842cd30-937e-430c-b903-daac81e90b69))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 4a44e8c8-addf-45c6-b4aa-ae80190bb455))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 8cec59d6-b83a-4f9b-8883-d9059e4d2491))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp be27fb48-1ced-442e-96ee-4abb96136c3a))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp e084d5b3-30c2-4104-af00-6d86a417a7a7))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp 2f0b2606-d7e1-45f7-bdd7-0a14596947d6))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp 63f95b1e-b740-4d19-873e-2f2dfe06e68b))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp 98e2820c-f2f3-4b60-a304-293abafd6590))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp 99143688-6167-4899-8afc-4a7e951a8e43))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp a2eb72a3-ddf9-4279-99b9-f11a681d2a0d))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp f7171d92-1ba6-4ce1-af8b-4102bcc4703e))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(J2-Pad20)") (pintype "passive") (tstamp f80f17a7-65dc-4f88-a77d-b9e5339c5e9c))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(R5-Pad2)") (pintype "passive") (tstamp e3554f49-f322-4ee4-b51c-c831d50e1fa6))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp f324c432-74a0-47c3-8d00-0e820559dd09)
    (at 172.466 121.92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico_tcs.kicad_sch")
    (property "Sheetname" "")
    (path "/3760c7e9-9161-4ca5-83d7-01ad3aa466b5")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 -2.37) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 33a397a5-0e6a-4e32-9572-7b4fd7425a63)
    )
    (fp_text value "1,2 Ohm" (at 5.08 2.794) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 431dd3c3-2ee9-454c-8683-d46ddff4f4b1)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9800b221-2c15-408d-9aa3-c6c78e4c0c61)
    )
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 34941a15-2a01-4f3c-aea4-8b37bdbf741f))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp 459f3649-b96f-4d5e-8438-74142ca5d268))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 5a4a0710-d8d4-42a5-bf60-26df9274a031))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp 98a49df6-d512-4d96-9177-d64be1fc468d))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp a7c8699a-c76c-47ea-a25b-a82764a0592a))
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp e9974b8b-8092-4d0c-aae9-c5a3d60c1aa6))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 06368f59-f6d0-45f0-a2a5-0c8242859dbf))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 0a20872d-4921-49b7-a625-cf7b94c7ea1b))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 8c2f085e-9ce8-4265-8709-6920fdf8598f))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp dcc59459-5416-483d-a2c3-c820200980b0))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp 0bcf22e8-1ab4-4604-b384-5a9b6381d26c))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp 26ff681e-0db4-4251-a25e-8cb7c9c701a4))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp 2ddb9641-a2c1-4895-9fbd-c89c98e4826f))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp 5843ccfa-b30e-4523-88ad-611d2a590e48))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp 67ad6131-29a1-4a52-8db3-244b8c4fa189))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp a88f5db3-9dc7-4ba3-81a2-bf2083c1e14a))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(R1-Pad1)") (pintype "passive") (tstamp 3df8f82e-f6b9-4766-93e4-447fee7e08e9))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(J1-Pad4)") (pintype "passive") (tstamp 8310a334-e7bf-4ed0-b897-a7f73877bae7))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 148.336 71.12) (end 213.36 132.588) (layer "Edge.Cuts") (width 0.1) (fill none) (tstamp f2f1b72b-8dff-4304-a6df-1ca95e6f332f))
  (gr_text "A" (at 190.116 121.457 -90) (layer "F.SilkS") (tstamp 2d527c2a-74d8-43b1-b4aa-0bb4b44489d5)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "VSYS" (at 188.458 74.955 -90) (layer "F.SilkS") (tstamp 3011dec2-ad75-4c8f-ac5c-61da4afeffa9)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "1" (at 206.522 88.9) (layer "F.SilkS") (tstamp 38d08193-45fa-441e-ab0b-3b784146789c)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "+" (at 206.118 121.203 -90) (layer "F.SilkS") (tstamp 49faaf3c-adca-450e-b40c-0f966ec073ac)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "DIN" (at 170.678 75.463 -90) (layer "F.SilkS") (tstamp 4b256ac6-aa7d-497b-bfa5-6dc249e7bbe9)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "CS" (at 175.758 76.225 -90) (layer "F.SilkS") (tstamp 4d50fb07-e63c-4a82-93b5-9a6d53242f9a)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "CLK" (at 173.218 75.463 -90) (layer "F.SilkS") (tstamp 6e7c9bb2-1b35-4bf0-9a85-d8149f96929b)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Keypad" (at 170.688 112.268) (layer "F.SilkS") (tstamp 702228ca-1091-4c3d-9fa1-e8268a243f1e)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "v1.4 © by Manuel Kamper 03.01.2023" (at 181.864 99.822) (layer "F.SilkS") (tstamp 7af876d3-55d7-4c3b-9390-2acb4b9874b2)
    (effects (font (size 1.5 1.5) (thickness 0.375)))
  )
  (gr_text "GND" (at 185.918 75.463 -90) (layer "F.SilkS") (tstamp 9f69c4fa-395a-45a2-9107-a434f4f273e7)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Raspberry Pico W" (at 166.37 89.408) (layer "F.SilkS") (tstamp a21f87b1-5861-4d76-8e4e-1111c068ed3f)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "SDA" (at 183.378 75.717 -90) (layer "F.SilkS") (tstamp b19eab01-cf8d-4ce7-b187-d6af67ef0db2)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "RST" (at 167.884 75.463 -90) (layer "F.SilkS") (tstamp b7ae6033-39ba-46f9-87cf-2a328dfdb0d1)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "TCS Bus" (at 186.56 114.091 90) (layer "F.SilkS") (tstamp c62a97c3-8dcd-4c91-80fb-bac28c82ab3a)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "-" (at 200.784 121.203 -90) (layer "F.SilkS") (tstamp d3b6a723-6efd-4967-a056-9f4f1a13a73a)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "1" (at 179.06 109.499) (layer "F.SilkS") (tstamp e1ddb436-d654-4476-b828-3f9a22df7091)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "B" (at 195.196 121.457 -90) (layer "F.SilkS") (tstamp e27191ae-f52e-4b45-9f4c-dc2c9dab9220)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "DC" (at 178.552 76.225 -90) (layer "F.SilkS") (tstamp e7089b67-48d2-4005-96fb-1b76ed2b8cde)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "Power" (at 211.198 114.091 90) (layer "F.SilkS") (tstamp efe88ede-8914-4fc8-ba8a-03c325675a5b)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "TCS<->FHEM" (at 182.118 94.996) (layer "F.SilkS") (tstamp f1e5e5ec-aadc-4698-b0c5-a7993f0287d1)
    (effects (font (size 4 4) (thickness 1)))
  )
  (gr_text "Display" (at 161.29 80.518) (layer "F.SilkS") (tstamp f5aa3ea8-f79b-4f97-a48c-b0120c4f853c)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )
  (gr_text "SCL" (at 180.838 75.717 -90) (layer "F.SilkS") (tstamp f985013a-eb4d-4db1-b272-30de7f5d8e15)
    (effects (font (size 1.5 1.5) (thickness 0.3)))
  )

  (segment (start 206.238 103.657) (end 206.238 112.955) (width 1.5) (layer "B.Cu") (net 1) (tstamp 42e1e233-8ae6-4759-836b-b6a51400bcce))
  (segment (start 206.238 112.955) (end 206.118 113.075) (width 0.25) (layer "B.Cu") (net 1) (tstamp 9015a8e4-0609-4e94-b9ac-625e34823d1c))
  (segment (start 185.918 82.54) (end 186.69 83.312) (width 1) (layer "B.Cu") (net 2) (tstamp 07cee603-880d-4ccc-b16f-a5327d29e56c))
  (segment (start 209.042 83.058) (end 209.042 89.916) (width 1) (layer "B.Cu") (net 2) (tstamp 18c33663-f3ad-48bf-8a87-5ee4d9c76720))
  (segment (start 154.178 129.54) (end 164.592 129.54) (width 1) (layer "B.Cu") (net 2) (tstamp 24eaec42-2ea9-4971-b838-c4fa2a7964f0))
  (segment (start 186.69 83.312) (end 208.788 83.312) (width 1) (layer "B.Cu") (net 2) (tstamp 2d9500aa-1520-425f-aa4b-12c34e9de504))
  (segment (start 151.892 127.254) (end 154.178 129.54) (width 1) (layer "B.Cu") (net 2) (tstamp 51538d3e-0ce8-489f-b476-6c9f194307b4))
  (segment (start 196.118 119.35) (end 196.118 113.075) (width 1) (layer "B.Cu") (net 2) (tstamp 69a8d5b6-e047-4c12-9aac-190da2331a89))
  (segment (start 164.592 129.54) (end 166.116 131.064) (width 1) (layer "B.Cu") (net 2) (tstamp 6e895883-ad5f-405e-bf52-76d3d318c56d))
  (segment (start 184.404 131.064) (end 196.118 119.35) (width 1) (layer "B.Cu") (net 2) (tstamp 769e7cb6-4e80-4a65-9fda-2cb015b0543d))
  (segment (start 209.042 89.916) (end 201.158 97.8) (width 1) (layer "B.Cu") (net 2) (tstamp 79e46d4d-7440-4a84-ba6a-c34696486ecb))
  (segment (start 201.158 97.8) (end 201.158 103.657) (width 1) (layer "B.Cu") (net 2) (tstamp 7d6a76f7-7b10-4fc0-87be-4629b54685f2))
  (segment (start 185.918 80.543) (end 185.918 82.54) (width 1) (layer "B.Cu") (net 2) (tstamp 99c7a8d4-7af8-4f03-b739-40bb248ed7e5))
  (segment (start 201.158 103.657) (end 201.158 113.035) (width 1.5) (layer "B.Cu") (net 2) (tstamp a8b2715a-6aaa-4002-a22e-6e1d4da6c3f5))
  (segment (start 201.158 113.035) (end 201.118 113.075) (width 0.25) (layer "B.Cu") (net 2) (tstamp cb5fa38f-2565-4d04-bce0-1ad670b24970))
  (segment (start 166.116 131.064) (end 184.404 131.064) (width 1) (layer "B.Cu") (net 2) (tstamp d3329713-1cb1-4b2f-9bbe-2c6d56c1bb6c))
  (segment (start 208.788 83.312) (end 209.042 83.058) (width 0.25) (layer "B.Cu") (net 2) (tstamp d54f4e71-3a98-40b9-947c-ffb5d26a2ad6))
  (segment (start 201.118 113.075) (end 196.118 113.075) (width 1.5) (layer "B.Cu") (net 2) (tstamp db8402cc-1faf-4ae2-b6e8-76644cab9031))
  (segment (start 183.378 80.543) (end 183.378 82.446604) (width 1) (layer "B.Cu") (net 9) (tstamp 5411f893-4fa9-44d4-bfe8-7effc1b4affe))
  (segment (start 183.378 82.446604) (end 185.918 84.986604) (width 1) (layer "B.Cu") (net 9) (tstamp 94a2edb9-a6bb-4d98-b9aa-fa7c7d1fd91e))
  (segment (start 185.918 84.986604) (end 185.918 85.877) (width 0.25) (layer "B.Cu") (net 9) (tstamp d001cdeb-8ee5-4ddd-857b-5fbfa547e448))
  (segment (start 175.758 103.657) (end 175.758 109.245) (width 1) (layer "B.Cu") (net 24) (tstamp df273d80-f766-4821-afa1-d53d0f3fe4a4))
  (segment (start 173.218 103.657) (end 173.218 109.245) (width 1) (layer "B.Cu") (net 25) (tstamp e5604d64-e77d-4b11-a930-b7de9d0de544))
  (segment (start 170.678 103.657) (end 170.678 109.245) (width 1) (layer "B.Cu") (net 26) (tstamp 66b47a5c-a6a8-44a8-a469-8296c52cd123))
  (segment (start 168.138 103.657) (end 168.138 109.245) (width 1) (layer "B.Cu") (net 27) (tstamp c0a73d3a-ee67-4cb9-bcfb-0d4d7f807201))
  (segment (start 165.598 103.657) (end 165.598 109.245) (width 1) (layer "B.Cu") (net 28) (tstamp 1ee8eaf2-0ddc-44aa-929e-b63e0b916aef))
  (segment (start 180.848 83.347) (end 180.848 82.55) (width 1) (layer "B.Cu") (net 29) (tstamp 3cacb502-63e5-4110-8325-6981ecdbf985))
  (segment (start 180.848 82.55) (end 180.838 82.54) (width 0.25) (layer "B.Cu") (net 29) (tstamp 3d8afa98-e88f-415f-9436-f3cad2755c3e))
  (segment (start 183.378 85.877) (end 180.848 83.347) (width 1) (layer "B.Cu") (net 29) (tstamp 95648a97-e7be-4d93-a05c-ed6dad82e16c))
  (segment (start 180.838 82.54) (end 180.838 80.543) (width 1) (layer "B.Cu") (net 29) (tstamp eab2a4f1-fde2-4273-ab8d-80fa8c426cb1))
  (segment (start 178.298 83.337) (end 178.298 80.543) (width 1) (layer "B.Cu") (net 30) (tstamp 27a4cca9-b3f0-42b0-a9ac-3bdb52033ca7))
  (segment (start 180.838 85.877) (end 178.298 83.337) (width 1) (layer "B.Cu") (net 30) (tstamp fc953ceb-0264-4050-9500-c96a277d65c8))
  (segment (start 178.298 85.877) (end 175.758 83.337) (width 1) (layer "B.Cu") (net 31) (tstamp 15c8458b-9a15-44f5-8e96-d42ab4a1d229))
  (segment (start 175.758 83.337) (end 175.758 80.543) (width 1) (layer "B.Cu") (net 31) (tstamp 6a3d22f5-ea44-4160-a85a-1b4c3211cdd9))
  (segment (start 173.218 80.543) (end 173.218 85.877) (width 1) (layer "B.Cu") (net 33) (tstamp ad0a0d55-fa21-4db8-bff6-9ec1b0a1ce47))
  (segment (start 170.678 80.543) (end 170.678 85.877) (width 1) (layer "B.Cu") (net 34) (tstamp d7f0eada-11af-4200-a754-c2b6a8f11f5d))
  (segment (start 168.138 80.543) (end 168.138 85.877) (width 1) (layer "B.Cu") (net 35) (tstamp a6ae4218-a35d-41f9-bf1c-3bf070d226fb))
  (segment (start 188.458 80.543) (end 210.337 80.543) (width 1) (layer "B.Cu") (net 36) (tstamp 1ebdee26-b588-472e-91f1-28df15dae5e6))
  (segment (start 210.82 81.026) (end 210.82 92.71) (width 1) (layer "B.Cu") (net 36) (tstamp 20f14679-c807-423c-8bcb-05f7e7d72ad0))
  (segment (start 210.82 92.71) (end 203.698 99.832) (width 1) (layer "B.Cu") (net 36) (tstamp 6b2d6311-b4f4-4bac-af8e-e0769a8437e6))
  (segment (start 210.337 80.543) (end 210.82 81.026) (width 1) (layer "B.Cu") (net 36) (tstamp e3025130-7ac0-444a-8f32-f918a0d5ec90))
  (segment (start 203.698 99.832) (end 203.698 103.657) (width 1) (layer "B.Cu") (net 36) (tstamp f9f2e295-7751-4312-817a-e26cf1ba9107))
  (segment (start 182.626 121.92) (end 182.626 127.762) (width 1) (layer "B.Cu") (net 52) (tstamp 5e21946d-2ef0-40dd-8610-ced0492de9a4))
  (segment (start 182.626 118.11) (end 182.626 121.92) (width 1) (layer "B.Cu") (net 52) (tstamp 7d49df2f-d535-41e4-a13a-4571f4ba7d1b))
  (segment (start 182.626 118.11) (end 186.083 118.11) (width 1) (layer "B.Cu") (net 52) (tstamp 942325a0-5c2e-47ef-8be5-cb4918e22936))
  (segment (start 186.083 118.11) (end 191.118 113.075) (width 1) (layer "B.Cu") (net 52) (tstamp f1323458-2e66-4509-ba0e-04fb3c367c23))
  (segment (start 160.782 109.474) (end 169.418 118.11) (width 1) (layer "B.Cu") (net 53) (tstamp 8f679325-8bfa-4acb-919d-77efef58fb05))
  (segment (start 172.466 118.11) (end 172.466 121.92) (width 1) (layer "B.Cu") (net 53) (tstamp 961cc31d-71bf-4997-b0f9-abcd14aabc89))
  (segment (start 159.512 109.474) (end 160.782 109.474) (width 1) (layer "B.Cu") (net 53) (tstamp a76d3ea1-a9cf-4b47-95c4-1ce9f0032b2d))
  (segment (start 169.418 118.11) (end 172.466 118.11) (width 1) (layer "B.Cu") (net 53) (tstamp f92fcf46-e4d7-4079-88a0-be9dbc2b02c7))
  (segment (start 153.162 108.204) (end 151.892 109.474) (width 1) (layer "B.Cu") (net 54) (tstamp 25e3f24e-a95b-4392-9dfb-47fd90c443a2))
  (segment (start 153.162 99.822) (end 153.162 108.204) (width 1) (layer "B.Cu") (net 54) (tstamp c34c6139-ffd3-41da-89b7-2c7cb4391222))
  (segment (start 156.947 85.877) (end 157.978 85.877) (width 1) (layer "B.Cu") (net 55) (tstamp 073f4a22-25d7-4399-a58c-36ddf191c3ec))
  (segment (start 153.162 89.662) (end 156.947 85.877) (width 1) (layer "B.Cu") (net 55) (tstamp 7331419c-8342-4479-8c76-7e139983539b))
  (segment (start 190.998 107.178) (end 190.998 103.657) (width 1) (layer "B.Cu") (net 56) (tstamp 21ef44e9-b02f-422b-8c12-302241a97393))
  (segment (start 164.592 119.38) (end 172.466 127.254) (width 1) (layer "B.Cu") (net 56) (tstamp 418db50a-a58c-4fb3-942b-fc9d4deda1e5))
  (segment (start 172.466 127.254) (end 172.466 127.762) (width 0.25) (layer "B.Cu") (net 56) (tstamp 5639f76b-eaaf-4787-a5f8-cb77caf72750))
  (segment (start 184.15 107.188) (end 191.008 107.188) (width 1) (layer "B.Cu") (net 56) (tstamp 87a129fb-e9e9-4a4f-9654-646e75bc2069))
  (segment (start 172.466 127.762) (end 177.292 122.936) (width 1) (layer "B.Cu") (net 56) (tstamp 87a4786d-7e65-477c-9de7-092043182a3d))
  (segment (start 177.292 114.046) (end 184.15 107.188) (width 1) (layer "B.Cu") (net 56) (tstamp 8f664266-1355-45bd-b9aa-9ffb81ae5c06))
  (segment (start 177.292 122.936) (end 177.292 114.046) (width 1) (layer "B.Cu") (net 56) (tstamp a4145759-6688-4c65-95bc-dd6358a9a810))
  (segment (start 191.008 107.188) (end 190.998 107.178) (width 0.25) (layer "B.Cu") (net 56) (tstamp eea977cd-98b7-4580-a7dd-37b439afae42))

)
